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	Purpose:
	To define the key terms used throughout the standard, providing a common understanding for implementing and maintaining an effective Occupational Health and Safety (OH&S) Management System. 


	Scope:
	This clause specified that the definitions of terms used in the Company’s OHSMS is limited to within the ISO 45001 standard itself.


	ISO Reference:
	MS ISO 45001:2018 Clause No. 3




	Revision History

	Revision No.
	Revision Date
	Originator
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	Definitions

	HIRARC
	Hazard Identification, Risk Assessment, and Risk Control

	SWMS
	Safe Work Method Statement

	PPE
	Personal Protective Equipment

	PTW
	Permit To Work



	Step
	Activity
	Responsibility
	Reference
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	MS ISO 45001:2018 Clause 3 - Terms And Definitions:

For the application of this OHSMS, the terms and definitions given in ISO 45001:2018 Clause 3.1 to 3.37 and general terms specified below shall apply.
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MS ISO 45001:2018 
OHSMS




	General Term
	Definition

	OH&S (Occupational Health & Safety)
	Conditions and factors that affect the health, safety, and well-being of workers and other interested parties.

	Hazard
	A source with the potential to cause injury or ill health.

	Risk
	The combination of the likelihood of occurrence of a hazardous event and the severity of injury or ill health that can be caused.

	Worker
	Person performing work or work-related activities under the control of the organization (including employees, subcontractors, agency staff, and other outsourced workers).

	Workplace
	Place under the control of the organization where a person needs to be or to go for work purposes.

	Incident
	Occurrence arising out of or in the course of work that could or does result in injury or ill health (including near misses).

	Interested Party
	Person or organization that can affect, be affected by, or perceive themselves to be affected by decisions or activities of the organization.


	Step
	Activity
	Responsibility
	Reference
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	Additional terms and definitions specific to the operation of M&E Contractors are provided below to enhance understanding and effective implementation of the OHSMS.

	IM
	



	M&E Contractor Term
	Definition

	HIRARC
	Hazard Identification, Risk Assessment, and Risk Control – A process used to identify potential hazards, assess associated risks, and implement appropriate controls.

	PPE
	Personal Protective Equipment – Safety gear provided to workers to minimize exposure to hazards (helmets, gloves, safety harness, etc.).

	Safe Work Method Statement (SWMS)
	A documented procedure detailing how specific high-risk activities are to be carried out safely.

	Permit to Work (PTW)
	Formal authorization process for high-risk activities (such as electrical isolation, confined space, or working at height).

	Subcontractor
	External party engaged by the company to perform specific works or services under the company's control.

	Safety & Health Officer (SHO)
	Competent person appointed to advise and assist the organization in matters relating to OH&S.

	Main Contractor
	The party awarding the contract to the M&E Contractor and having overall responsibility for the project site.
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	Abbreviations used in this OHSMS listed as per Annex A shall also apply.

	IM
	>>> Annex A – Abbreviation
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